IDApp will communicate with a bridge executable over the named pipe. The executable will then decrypt the video file in blocks and will write it to some temp locations and pass it to UI. The UI will then read the file from that location.

The executable will create the cached video file at random location and will pass it to the UI.

More can be thought on the encryption of the communication b/w IDApp and bridge executable.